**STANDARD EQUIPMENT**

Power – assisted steering system

12v DC/240v AC electrical system

220/240v shore power with 35-amp float battery charger

Remote control electric anchor winch

Electro-hydraulic trim tabs

VHF with DSC R/T

Speed and distance log

Echo Sounder with alarm

Remote control with alarm

Remote control searchlight

Combination microwave/ conventional oven grill

Refrigerator with deep freeze compartment

Cockpit wet bar including sink and top loading cool

Box (optional electric barbecue)

Electric quiet flush toilet

Saloon stereo CD/radio/MP3 and cockpit speakers

Teak-laid cockpit and transom platform

Hot and cold transom shower

Tonneau cover

Cockpit sunroof with electric operation

Twin Volvo D6-330DP (2x330 mhp)- Stern drive

Bow thruster

**HULL COLOR**

White

**INTERIOR FURNITURE**

Serotina Cherry wood satin finish (teak galley floor is standard)

Saloon to have timber floor in place of carpet

**LAYOUT**

Sunbed option- aft seat extension with sliding backrest so as to covert to sunbed

**FACILITY**
Loudspeakers linked to saloon radio fitted in forward coach roof

**NAVIGATION**
The V39 is fitted with Ray marine i70 color multifunction display (for
speed, distance, trip, depth, depth alarm, water temperature etc,
Ray marine e125 Chart plotter/GPS with extemal GPS and 12.1" brilliant
color multifunction display

Automatic pilot(Ray marine p70R with color display and rate gyro)

**AIRCONDITIONING**
Air-conditioning, 2 x 12,000btu units (with reverse cycle heating)
supplying saloon, forward & aft cabins and bathroom
Rccommended generator: 4Kw
HOLDING TANK/TOILETS

SYSTEM 2: Toilet discharging into the holding tank but also having the
ability to discharge directly overboard via a Y valve fitted in the
Discharge lines. The holding tank has electric overboard discharge as
well as reserve manual and dockside discharge arrangements

EXTERIOR UPHOLSTERY/CANVAS COVERS
Foredeck sunbed cushions in white vinyl with contrast paneling to
upstand of cushions
Charcoal grey umbrella anti reflective cover to horizontal area behind
Windscreen(easily removable, located by poppers)
Black mesh windscreen covers
Full height cockpit cover in white sunbrella with removable sides and
Back( on telescopic stainless steel frame& vertical supports) in place of
Standard tonneau cover top acts as sun awning when sides are removed)

Aft cabin to have sliding double berth conversion
Heat reflective blind (fitted in place with suction caps) to saloon overhead
Skylight with storage bag
**GALLEY**Midnight skype galley top
COLOR SCHEME
Additional charge for ultra-leather for saloon sofa
**DECK HARDWARE**
Note: the maximum weight allowed for a tender, including outboard, is
100kg to ensure satisfactory handling and performance)
Sliding side window at helm position (aperture 36cm H x 38cm L)

Transom platform to have electro-hydraulic lift mechanism
(Note: The safe working load of the platform is 250kg, but the maximum
weight of tender and outboard remain at 100kg) raised teak deck at helm position

**GENERATOR**
Price includes shore support changeover switch and remote control panel
ONAN 4 Kw/50Hz generator (with hydro hush exhaust system and sound
shield)

**ELECTRICAL**Continental 220v/240v sockets
Electric hob (2 burner) in place of standard gas hob and gas
System
Electric BBQ in cockpit wet bar
12v Exterior splash proof power point (cach - specify location)
Underwater transom lights (2 AMPHIBIAN A6 LED)
Blue low level cockpit and bathing platform led. Lights

AUDIO VISUAL & COMMUNICATIONS
Saloon -26" LED TV when this option is requested the standard
iPod/MP3/Radio is upgraded to FusionIP700 with video &Bluetooth